SECTION 10 14 19

SPECIAL GRAPHICS

Display hidden notes to specifier. (Don't know how? Click Here) 

** NOTE TO SPECIFIER ** Corpus Christi Stamp Works Inc. DBA/ National Signage Affiliates; . This section is based on the products of Corpus Christi Stamp Works Inc. DBA/ National Signage Affiliates, which is located at: P. O. Box 2189 502 S. Staples (78401) Corpus Christi, TX 78403 Toll Free: 800-322-4515 Fax: 800-354-6416 Email: sales@ccstampworks.com Web Site: www.ccswsignsystems.com 
PART  1	  GENERAL
1.1 		SECTION INCLUDES
** NOTE TO SPECIFIER ** Delete items below not required for project.
A.		Dimensional Letters 
1.            Flat Cut Metal
2.	     Flat Cut Acrylic
3.	     Flat Cut Foam
4.	     Cast Metal
5.	     Formed Plastic
6.            Fabricated Metal Letters
1.2 		RELATED SECTIONS
** NOTE TO SPECIFIER ** Delete any sections below not relevant to this project; add others as required. 
A.		Section 01100 – Administrative Requirements.
B.	          Section 06200 - Finish Carpentry.
C.		Section 09200 - Plaster and Gypsum Board.
D.		Section 09700 - Wall Finishes.
E.		Section 10410 - Directories.
F.		Section 16500 - Lighting.
1.3 		REFERENCES
** NOTE TO SPECIFIER ** Delete references from the list below that are not actually required by the text of the edited section. 
A.		Americans with Disabilities Act (ADA).
B.		American National Standards Institute (ANSI):
1.		ANSI A117.1 - Accessible and Usable Buildings and Facilities Standards.
1.4 		SUBMITTALS
A.		Submit under provisions of Section 01300.
B.		Product Data: Manufacturer's data sheets on each product to be installed.
C.		Shop Drawings: Shop drawings with letter style, dimensions, materials, finishes and general layout for each sign type, with sizes, edge and corner treatment, and mounting methods shown.
** NOTE TO SPECIFIER ** Delete if selection samples have already been selected.
D.		Selection Samples: For each finish specified, two complete sets of color chips representing manufacturer's full range of available colors, patterns and finishes. 
** NOTE TO SPECIFIER ** Delete if verification sample not required.
E.		Verification Samples: For each finish product specified, one full-size sign or typical letter representing actual product, color, patterns, and finishes. Include method of raised symbols and copy.
** NOTE TO SPECIFIER ** Delete if not required.
F.	     Sustainable Design Submittals:
1.	     Recycled Content – Provide documentation from Manufacturer verifying percentage of recycled and post-consumer content.
2.	     Regional Materials – Provide documentation form manufacturer/distributor showing location where materials were obtained from for each component.
1.5 		QUALITY ASSURANCE
A.		Manufacturer Qualifications: Manufacturer shall have five years experience manufacturing and fabricating products of similar type and scope as those specified in this section.
** NOTE TO SPECIFIER ** Include a mock-up if the project size and/or quality warrant taking such a precaution. The following is one example of how a mock-up on a large project might be specified. When deciding on the extent of the mock-up, consider all the major different types of work on the project. 
B.		Mock-Up: Provide a mock-up or sample for evaluation of Workmanship, Color, Finish, and Font.
1.		Finish areas designated by Architect.
2.		Do not proceed with remaining work until workmanship, color, and sheen are approved by Architect.
3.		Refinish mock-up or sample as required to produce acceptable work.
1.6 		DELIVERY, STORAGE, AND HANDLING
A.		Comply with manufacturer's recommendations for delivery, storage and handling.
B.		Materials shall be delivered to the location in unopened, labeled factory containers. Upon delivery, materials shall be inspected for damage. Deficient materials shall not be used.
1.7 		PROJECT CONDITIONS
A.		Maintain environmental conditions (temperature, humidity, and ventilation) within limits recommended by manufacturer for optimum results. Do not install products under environmental conditions outside manufacturer's absolute limits.
PART  2	  PRODUCTS
2.1 		MANUFACTURERS
A.		Acceptable Manufacturer: Corpus Christi Stamp Works Inc. DBA/ National Signage Affiliates, which is located at: P. O. Box 2189 502 S. Staples (78401) ; Corpus Christi, TX 78403; Toll Free Tel: 800-322-4515; Email:  (sales@ccstampworks.com); Web: www.ccswsignsystems.com 
** NOTE TO SPECIFIER ** Delete one of the following two paragraphs; coordinate with requirements of Division 1 section on product options and substitutions. 
B.		Substitutions: Not permitted.
C.		Requests for substitutions will be considered in accordance with provisions of Section 01600.
2.2 		SPECIAL GRAPHICS
** NOTE TO SPECIFIER ** Custom sizes and mounting mechanisms available. Delete if not required. 
** NOTE TO SPECIFIER ** Delete if not required. 
A.		Dimensional Letters and Logos: 
1.		Materials
a.	     Aluminum Plate
b.	     Cast Aluminum
c.	     Stainless Steel
d.	     Brass
e.	     Cast Brass
f.	      Bronze
g.	     Cast Bronze
h.	     Copper
i.	      Formed Plastic
j.	      Flat cut Plastic
k.	     Flat cut Foam
l.	      Foam with laminate face
m.	     Foam with plastic face
n.	     Foam with metal face.
2.	    Accessories
a.	     Anchors: Type best suited for application
b.	     Adhesive: Silicone based.
c.	     Tape.
3.	   Fabrication
a.	     Fabricate letters in accordance with approved Shop Drawings.
b.	     Cut letters from ____ inch thick Aluminum
c.	     Cut letters from ____ inch thick stainless steel.
d.	     Cut letters from ____ inch thick bronze
e.	     Cut letters from ____ inch thick brass
f.	      Cut letters from ____ inch thick plastic
g.	     Cut letters from ____ inch thick foam.
h.	     Cast letters from aluminum free from pits, gas holes, and warped surfaces.
i.	      Form letters from plastic.
j.	      Hand tool to sharp clean edges
k.	     Character Style:________
l.	      Height: ____ inches
m.	    Mounting style: Projected
n.	     Mounting style: Surface
o.	     Mounting style: Bottom.
p.	     Mounting style: Bar.
q.	     Mounting style: _____
4.	     Finishes:
a.	     Natural Satin
b.	     Polished
c.	     Clear Anodized
d.	     Painted
1)	    Color: _____
e.	     Plastic Color: _____
** NOTE TO SPECIFIER ** Delete if not required. 
** NOTE TO SPECIFIER ** Delete if not required. 
PART  3	  EXECUTION
3.1 		EXAMINATION
A.		Installer shall examine signs for defects, damage, and compliance with specifications.  Installation shall not proceed until satisfactory conditions are achieved.
B.	     Inspect conditions of substrate and other conditions which may affect installation of signage. 
C.		Do not begin installation until substrates are within manufacturer's specified tolerances and have been prepared in accordance with manufacturer's instructions.
D.		If substrate preparation is the responsibility of another installer, do not proceed with installation. Notify Architect of any unsatisfactory conditions immediately. 
E.		Commencement of work is deemed as acceptance of installation conditions.
3.2 		PREPARATION
A.		Verify mounting heights and locations for signage will comply with specified requirements, including accessibility requirements.
B.		Prepare surfaces using the methods recommended by the manufacturer for achieving the best result for the substrate under the project conditions. Clean mounting locations of dirt, dust, grease or similar conditions that would prevent proper installation.
3.3 		INSTALLATION
A.		Install in accordance with manufacturer's printed installation instructions, and in proper relationship with adjacent work.
B.	  Use mounting methods and fasteners as recommended by the manufacturer.
** NOTE TO SPECIFIER ** The following paragraph is standard for room identification signage. Delete if not required. 
C.		Install interior room identification signage by means of double sided tape and silicone, installed within 60 inches (1524 mm) of finished floor to center of sign on the wall adjacent to the latch side of the door in accordance with ADA requirements, unless otherwise noted. Where there is no wall space, including double leaf doors, sign shall be placed on the nearest adjacent wall.
D.	  Set level, plumb, rigid and at heights indicated with surfaces free from defects.
3.4 		PROTECTION
A.		Protect installed products until completion of project.
B.		Touch-up, repair or replace damaged products before Substantial Completion.

END OF SECTION